kWh/kW - Year 1 |

The kilowatt-hour per kilowatt-year metric is the annual electric output in year one E OutputYear1 divided by the system capacity P SystemCapacity. For photovoltaic systems, the system capacity is the Array Power on the Array page. For concentrating solar power systems, the system capacity is the Rated Turbine Net Capacity on the Power Block page. Where,
E OutputYear1 (AC kWh/year) | The total annual electric generation in the first year of operation reported on the Metrics table, and in the year one column of the project cash flow.
P SystemCapacity (DC kW) | The system's rated capacity expressed in kilowatts (see table below).
The system capacity depends on technology being modeled. Note that Solar Advisor converts the capacity value to kW before using it in the calculation. Table 39. Rated system capacity values for each technology.
Technology | System Capacity | Input Page
PV SAM Performance Models | Total Array Power (Wdc) | Array
PV PVWatts | DC Rating (kW) | PVWatts Solar Array
CSP Parabolic Trough | Rated Turbine Net Capacity (MWe) | Power Block
CSP Power Tower | Nameplate Capacity (MWe) | Power Cycle
CSP Dish Stirling | Total Capacity (kW) | Solar Field
Generic Fossil | Nameplate Capacity (kWe) | Fossil Plant